**Platform assembly**

**1**-Lay out tubes as in figure 1, so your finish dimensions will be 76” length and 32” wide

**2**- use the sheet metal screws to assemble the corner brackets to the rail tubes Figure 2. 

 Fig 1

 Fig 2

**3**- make sure that all bracket screws are put in (4) in each bracket

**4**- center supprt tube should be placed so your top material ( **not included** ) will be well supported when attached

**5**- attach your mattress support to the top of the headboard side of the platform , to keep mattress in place

**6**-attach your material to the tube framework to complete the platform